|  |
| --- |
| **طرح نگهداشت و افزایش تولید 27 مخزن** |
| **MTO FOR EARTHING & LIGHTNING SYSTEMS****نگهداشت و افزایش تولید میدان نفتی بینک** |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
| D00 | Oct. 2022 | IFI | H.Shakiba | M.Fakharian | M.Mehrshad |  |
| **Rev.** | **Date** | **Purpose of Issue/Status** | **Prepared by:** | **Checked by:** | **Approved by:** | **CLIENT Approval** |
| **Class:3** | **CLIENT Doc. Number: F8Z-709073** |
| **Status:** | **IDC: Inter-Discipline Check****IFC: Issued For Comment** **IFA: Issued For Approval****AFD: Approved For Design** **AFC: Approved For Construction** **AFP: Approved For Purchase****AFQ: Approved For Quotation** **IFI: Issued For Information****AB-R: As-Built for CLIENT Review** **AB-A: As-Built –Approved** |

**REVISION RECORD SHEET**

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **PAGE** | **D00** | **D01** | **D02** | **D03** | **D04** |  | **PAGE** | **D00** | **D01** | **D02** | **D03** | **D04** |
| **1** | X |  |  |  |  | **51** |  |  |  |  |  |
| **2** | X |  |  |  |  | **52** |  |  |  |  |  |
| **3** | X |  |  |  |  | **53** |  |  |  |  |  |
| **4** | X |  |  |  |  | **54** |  |  |  |  |  |
| **5** | X |  |  |  |  | **55** |  |  |  |  |  |
| **6** | X |  |  |  |  | **56** |  |  |  |  |  |
| **7** |  |  |  |  |  | **57** |  |  |  |  |  |
| **8** |  |  |  |  |  | **58** |  |  |  |  |  |
| **9** |  |  |  |  |  | **59** |  |  |  |  |  |
| **10** |  |  |  |  |  | **60** |  |  |  |  |  |
| **11** |  |  |  |  |  | **61** |  |  |  |  |  |
| **12** |  |  |  |  |  | **62** |  |  |  |  |  |
| **13** |  |  |  |  |  | **63** |  |  |  |  |  |
| **14** |  |  |  |  |  | **64** |  |  |  |  |  |
| **15** |  |  |  |  |  | **65** |  |  |  |  |  |
| **16** |  |  |  |  |  | **66** |  |  |  |  |  |
| **17** |  |  |  |  |  | **67** |  |  |  |  |  |
| **18** |  |  |  |  |  | **68** |  |  |  |  |  |
| **19** |  |  |  |  |  | **69** |  |  |  |  |  |
| **20** |  |  |  |  |  | **70** |  |  |  |  |  |
| **21** |  |  |  |  |  | **71** |  |  |  |  |  |
| **22** |  |  |  |  |  | **72** |  |  |  |  |  |
| **23** |  |  |  |  |  | **73** |  |  |  |  |  |
| **24** |  |  |  |  |  | **74** |  |  |  |  |  |
| **25** |  |  |  |  |  | **75** |  |  |  |  |  |
| **26** |  |  |  |  |  | **76** |  |  |  |  |  |
| **27** |  |  |  |  |  | **77** |  |  |  |  |  |
| **28** |  |  |  |  |  | **78** |  |  |  |  |  |
| **29** |  |  |  |  |  | **79** |  |  |  |  |  |
| **30** |  |  |  |  |  | **80** |  |  |  |  |  |
| **31** |  |  |  |  |  | **81** |  |  |  |  |  |
| **32** |  |  |  |  |  | **82** |  |  |  |  |  |
| **33** |  |  |  |  |  | **83** |  |  |  |  |  |
| **34** |  |  |  |  |  | **84** |  |  |  |  |  |
| **35** |  |  |  |  |  | **85** |  |  |  |  |  |
| **36** |  |  |  |  |  | **86** |  |  |  |  |  |
| **37** |  |  |  |  |  | **87** |  |  |  |  |  |
| **38** |  |  |  |  |  | **88** |  |  |  |  |  |
| **39** |  |  |  |  |  | **89** |  |  |  |  |  |
| **40** |  |  |  |  |  | **90** |  |  |  |  |  |
| **41** |  |  |  |  |  | **91** |  |  |  |  |  |
| **42** |  |  |  |  |  | **92** |  |  |  |  |  |
| **43** |  |  |  |  |  | **93** |  |  |  |  |  |
| **44** |  |  |  |  |  | **94** |  |  |  |  |  |
| **45** |  |  |  |  |  | **95** |  |  |  |  |  |
| **46** |  |  |  |  |  | **96** |  |  |  |  |  |
| **47** |  |  |  |  |  | **97** |  |  |  |  |  |
| **48** |  |  |  |  |  | **98** |  |  |  |  |  |
| **49** |  |  |  |  |  | **99** |  |  |  |  |  |
| **50** |  |  |  |  |  | **100** |  |  |  |  |  |

**Bill of Material**

| **Overall Earthing System (BK-GCS-PEDCO-120-EL-PY-0001)** |
| --- |
| **Item** | **Description** | **Unit** | **Earthing** | **Lightning** | **Spare** | **Total** |
|  | Bare Round Earthing Copper Conductor 70 mm2 | m | 960 | 0 | 40 | **1000** |
|  | Bare Round Earthing Copper Conductor 240 mm2 | m | 275 | 0 | 25 | **300** |
|  | Earthing Copper Wire, G/Y PVC Insulated 16 mm2 | m | 1110 | 0 | 4090 | **1200** |
|  | Earthing Copper Wire, G/Y PVC Insulated 35 mm2 | m | 755 | 0 | 45 | **800** |
|  | Earthing Copper Wire, G/Y PVC Insulated 70 mm2 | m | 555 | 0 | 45 | **600** |
|  | Earthing Copper Wire, G/Y PVC Insulated 300 mm2 | m | 30 | 0 | 20 | **50** |
|  | Stainless Steel 316L/Copper Earthing Rod with 19 mm Diameter and 2x1.5 m Length (One End Sharp, One End Flat) With All Accessories. | Set. | 4 | 0 | 1 | **5** |
|  | Stainless Steel 316L /Copper Earthing Rod with 19 mm Diameter and 2x1.5m Length (One End Sharp, One End Flat) With All Accessories. &Test Earth Pit | Set. | 6 | 0 | 0 | **6** |
|  | Copper Clamp for Connecting Round Conductor Size of 70 mm2 to Earth Rod | No | 7 | 0 | 1 | **8** |
|  | Copper Clamp for Connecting Round Conductor Size of 300 mm2 to Earth Rod | No. | 3 | 0 | 1 | **4** |
|  | Tinned Copper Earth Bar with disconnect link on both end with 10 Holes, HDG Fixing Base , "Ω" Base, | Set. | 11 | 0 | 1 | **12** |
|  | Crimp Type Earthing Terminal Lug 300 mm2, Tinned Copper Type (With Suitable Bolt & Nut With 1-Spring,2-Flat Washers, Size M12, tin plated or bronze) | No. | 3 | 0 | 2 | **10** |
|  | Crimp Type Earthing Terminal Lug 240 mm2, Tinned Copper Type (With Suitable Bolt & Nut With 1-Spring,2-Flat Washers, Size M12, tin plated or bronze) | No. | 8 | 0 | 2 | **10** |
|  | Crimp Type Earthing Terminal Lug 70 mm2, Tinned Copper Type (With Suitable Bolt & Nut With 1-Spring,2-Flat Washers, Size M12, tin plated or bronze | No. | 31 | 0 | 4 | **35** |
|  | Crimp Type Earthing Terminal Lug 35 mm2, Tinned Copper Type (With Suitable Bolt & Nut With 1-Spring,2-Flat Washers, Size M12, tin plated or bronze | No. | 41 | 0 | 4 | **45** |
|  | Crimp Type Earthing Terminal Lug 16 mm2, Tinned Copper Type (With Suitable Bolt & Nut With 1-Spring,2-Flat Washers, Size M12, tin plated or bronze | No. | 48 | 0 | 2 | **50** |
|  | Exothermic Mould for T Connection 240/300/240 mm2 | Set. | 1 | 0 | 0 | **1** |
|  | Exothermic Mould for T Connection 240/240/240 mm2 | Set. | 1 | 0 | 0 | **1** |
|  | Exothermic Mould for T Connection240/70/240 mm2 | Set. | 2 | 0 | 0 | **2** |
|  | Exothermic Mould for T Connection240/35/240 mm2 | Set. | 1 | 0 | 0 | **1** |
|  | Exothermic Mould for T Connection240/16/240 mm2 | Set. | 1 | 0 | 0 | **1** |
|  | Exothermic Mould for T Connection70/70/70 mm2 | Set. | 5 | 0 | 0 | **5** |
|  | Exothermic Mould for T Connection70/35/70 mm2 | Set. | 4 | 0 | 0 | **4** |
|  | Exothermic Mould for T Connection70/16/70 mm2 | Set. | 4 | 0 | 0 | **4** |
|  | Exothermic Welding Powder Suitable for 3 Ways Connections240/300/240 including disc and starter | No. | 6 | 0 | 0 | **6** |
|  | Exothermic Welding Powder Suitable for 3 Ways Connections240/240/240 including disc and starter | No. | 4 | 0 | 0 | **4** |
|  | Exothermic Welding Powder Suitable for 3 Ways Connections 240/70/240 including disc and starter | No. | 17 | 0 | 1 | **18** |
|  | Exothermic Welding Powder Suitable for 3 Ways Connections 240/35/240 including disc and starter | No. | 6 | 0 | 0 | **6** |
|  | Exothermic Welding Powder Suitable for 3 Ways Connections 240/16/240 including disc and starter | No. | 2 | 0 | 0 | **2** |
|  | Exothermic Welding Powder Suitable for 3 Ways Connections 70/70/70 including disc and starter | No. | 34 | 0 | 1 | **35** |
|  | Exothermic Welding Powder Suitable for 3 Ways Connections 70/35/70 including disc and starter | No. | 30 | 0 | 1 | **31** |
|  | Exothermic Welding Powder Suitable for 3 Ways Connections 70/16/70 including disc and starter | No. | 32 | 0 | 1 | **32** |
|  | Installation tools kit for thermo weld connection comprising flint gun, glove, scraper & brush | Set | 1 | 0 | **1** |

| **Earthing & Lightning Layout for Building & Shelter (BK-GCS-PEDCO-120-EL-PY-0002)** |
| --- |
| **Item** | **Description** | **Unit** | **Earthing** | **Lightning** | **Spare** | **Total** |
|  | Bare Round Earthing Copper Conductor 70 mm2 | m | 50 | 0 | 10 | **60** |
|  | Earthing Copper Wire, G/Y PVC Insulated 35 mm2 | m | 15 | 0 | 5 | **20** |
|  | Earthing Copper Wire, G/Y PVC Insulated 70 mm2 | m | 595 | 0 | 55 | **650** |
|  | Earthing Copper Wire, B/Y PVC Insulated 70 mm2 | m | 55 | 0 | 15 | **702** |
|  | Stainless Steel 316L/Copper Earthing Rod with 19 mm Diameter and 2x1.5 m Length (One End Sharp, One End Flat) With All Accessories. | Set. | 0 | 24 | 1 | **25** |
|  | Stainless Steel 316L/Copper Earthing Rod with 19 mm Diameter and 1 m Length (One End Sharp, One End Flat) With All Accessories. | Set. | 12 | 0 | 1 | **13** |
|  | Stainless Steel 316L/Copper Earthing Rod with 19 mm Diameter and 1 m Length (One End Sharp, One End Flat) With All Accessories & Test Pit | Set. | 2 | 0 | 0 | **2** |
|  | Stainless Steel 316L/Copper Earthing Rod with 19 mm Diameter and 2x1.5 m Length (One End Sharp, One End Flat) With All Accessories & Test Pit | Set. | 0 | 4 | 0 | **4** |
|  | Copper Clamp for Connecting Round Conductor Size of 70 mm2 to Earth Rod | No | 14 | 0 | 1 | **15** |
|  | Copper Clamp for Connecting Round Conductor Size of 70 mm2 to Earth Rod | No | 0 | 28 | 3 | **31** |
|  | Tinned Copper Earth Bar with disconnect link on both end with 10 Holes, HDG Fixing Base , "Ω" Base, | Set. | 6 | 0 | 1 | **7** |
|  | Crimp Type Earthing Terminal Lug 70 mm2, Tinned Copper Type (With Suitable Bolt & Nut With 1-Spring,2-Flat Washers, Size M12, tin plated or bronze | No. | 12 | 0 | 1 | **13** |
|  | Crimp Type Earthing Terminal Lug 35 mm2, Tinned Copper Type (With Suitable Bolt & Nut With 1-Spring,2-Flat Washers, Size M12, tin plated or bronze | No. | 1 | 0 | 1 | **2** |
|  | Exothermic Mould for T Connection70/70/70 mm2 | Set. | 3 | 6 | 1 | **10** |
|  | Exothermic Welding Powder Suitable for 3 Ways Connections 70/70/70 including disc and starter | No. | 19 | 34 | 2 | **55** |
|  | Copper nickel Chrome Coated Air Terminal Class I, 19mm Diameter, 0.6m Length with, with all accessories Thread | Set. | 0 | 19 | 1 | **20** |
|  | Air Terminal Saddle Suitable for 0.6m Air Terminal, also Suitable for Connecting 25x3 mm2 Flat tape to rod | Set. | 0 | 19 | 1 | **20** |
|  | Flat Copper Tape with 25 mm Width and 3 mm Thickness | m. | 0 | 461 | 39 | **500** |
|  | Clip Suitable for 25\*3 mm2 Flat Copper Tape fixing, with all accessories | No. | 0 | 233 | 17 | **250** |
|  | Test Link Suitable for 25\*3 mm2 Copper Tape and 70 mm2 Round Wire, with all accessories | Set. | 0 | 14 | 1 | **15** |
|  | Installation tools kit for thermo weld connection comprising flint gun, glove, scraper & brush | Set | 1 | 1 | Set |

| **Earthing Layout for Desalting Unit (BK-GCS-PEDCO-120-EL-PY-0014)** |
| --- |
| **Item** | **Description** | **Unit** | **Earthing** | **Lightning** | **Spare** | **Total** |
|  | Earthing Copper Wire, G/Y PVC Insulated 70 mm2 | m | 50 | 0 | 0 | **50** |
|  | Tinned Copper Earth Bar with disconnect link on both end with 10 Holes, HDG Fixing Base , "Ω" Base, | Set. | 6 | 0 | 1 | **7** |
|  | Exothermic Welding Powder Suitable for 3 Ways Connections 70/70/70 including disc and starter | Set. | 1 | 0 | 0 | **1** |

| **Earthing Layout for Production Unit (BK-GCS-PEDCO-120-EL-PY-0015)** |
| --- |
| **Item** | **Description** | **Unit** | **Earthing** | **Lightning** | **Spare** | **Total** |
|  | Earthing Copper Wire, G/Y PVC Insulated 70 mm2 | m | 50 | 0 | 0 | **50** |
|  | Tinned Copper Earth Bar with disconnect link on both end with 10 Holes, HDG Fixing Base , "Ω" Base, | Set. | 6 | 0 | 1 | **7** |
|  | Exothermic Welding Powder Suitable for 3 Ways Connections 70/70/70 including disc and starter | Set. | 1 | 0 | 0 | **1** |

1. This document shall be Based on below references:
* Calculation Note for Earthing & Lightning System BK-GCS-PEDCO-120-EL-CN-0006
* Overall Earthing Layout BK-GCS-PEDCO-120-EL-PY-0001
* Earthing & Lightning Layout for Building & Shelter BK-GCS-PEDCO-120-EL-PY-0002
* Earthing Layout for Desalting Unit BK-GCS-PEDCO-120-EL-PY-0014
* Earthing Layout for Production Unit BK-GCS-PEDCO-120-EL-PY-0015