|  |
| --- |
| **طرح نگهداشت و افزایش تولید 27 مخزن** |
| **PROCESS ELECTRICAL LOAD LIST** **نگهداشت و افزایش تولید میدان نفتی بینک** |
|  |  |  |  |  |  |  |
| D03 | JAN.2023 | IFA | M.Aryafar | M.Fakharian | M.Mehrshad |  |
| D02 | AUG.2022 | IFA | M.Aryafar | M.Fakharian | M.Mehrshad |  |
| D01 | MAR.2022 | IFA | M.Aryafar | M.Fakharian | M.Mehrshad |  |
| D00 | JAN.2022 | IFC | M.Aryafar | M.Fakharian | M.Mehrshad |  |
| **Rev.** | **Date** | **Purpose of Issue/Status** | **Prepared by:** | **Checked by:** | **Approved by:** | **CLIENT Approval** |
| **Class:** 2 | **CLIENT Doc. Number:** F0Z-708808 |
| **Status:** | **IDC: Inter-Discipline Check****IFC: Issued For Comment** **IFA: Issued For Approval****AFD: Approved For Design** **AFC: Approved For Construction** **AFP: Approved For Purchase****AFQ:** Approved For Quotation **IFI: Issued For Information****AB-R: As-Built for CLIENT Review** **AB-A: As-Built –Approved** |

**REVISION RECORD SHEET**

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **PAGE** | **D00** | **D01** | **D02** | **D03** | **D04** |  | **PAGE** | **D00** | **D01** | **D02** | **D03** | **D04** |
| **1** | X |  |  |  |  | **66** |  |  |  |  |  |
| **2** | X |  |  |  |  | **67** |  |  |  |  |  |
| **3** | X |  |  |  |  | **68** |  |  |  |  |  |
| **4** | X |  |  |  |  | **69** |  |  |  |  |  |
| **5** | X |  |  |  |  | **70** |  |  |  |  |  |
| **6** | X | X | X | X |  | **71** |  |  |  |  |  |
| **7** |  |  |  |  |  | **72** |  |  |  |  |  |
| **8** |  |  |  |  |  | **73** |  |  |  |  |  |
| **9** |  |  |  |  |  | **74** |  |  |  |  |  |
| **10** |  |  |  |  |  | **75** |  |  |  |  |  |
| **11** |  |  |  |  |  | **76** |  |  |  |  |  |
| **12** |  |  |  |  |  | **77** |  |  |  |  |  |
| **13** |  |  |  |  |  | **78** |  |  |  |  |  |
| **14** |  |  |  |  |  | **79** |  |  |  |  |  |
| **15** |  |  |  |  |  | **80** |  |  |  |  |  |
| **16** |  |  |  |  |  | **81** |  |  |  |  |  |
| **17** |  |  |  |  |  | **82** |  |  |  |  |  |
| **18** |  |  |  |  |  | **83** |  |  |  |  |  |
| **19** |  |  |  |  |  | **84** |  |  |  |  |  |
| **20** |  |  |  |  |  | **85** |  |  |  |  |  |
| **21** |  |  |  |  |  | **86** |  |  |  |  |  |
| **22** |  |  |  |  |  | **87** |  |  |  |  |  |
| **23** |  |  |  |  |  | **88** |  |  |  |  |  |
| **24** |  |  |  |  |  | **89** |  |  |  |  |  |
| **25** |  |  |  |  |  | **90** |  |  |  |  |  |
| **26** |  |  |  |  |  | **91** |  |  |  |  |  |
| **27** |  |  |  |  |  | **92** |  |  |  |  |  |
| **28** |  |  |  |  |  | **93** |  |  |  |  |  |
| **29** |  |  |  |  |  | **94** |  |  |  |  |  |
| **30** |  |  |  |  |  | **95** |  |  |  |  |  |
| **31** |  |  |  |  |  | **96** |  |  |  |  |  |
| **32** |  |  |  |  |  | **97** |  |  |  |  |  |
| **33** |  |  |  |  |  | **98** |  |  |  |  |  |
| **34** |  |  |  |  |  | **99** |  |  |  |  |  |
| **35** |  |  |  |  |  | **100** |  |  |  |  |  |
| **36** |  |  |  |  |  | **101** |  |  |  |  |  |
| **37** |  |  |  |  |  | **102** |  |  |  |  |  |
| **38** |  |  |  |  |  | **103** |  |  |  |  |  |
| **39** |  |  |  |  |  | **104** |  |  |  |  |  |
| **40** |  |  |  |  |  | **105** |  |  |  |  |  |
| **41** |  |  |  |  |  | **106** |  |  |  |  |  |
| **42** |  |  |  |  |  | **107** |  |  |  |  |  |
| **43** |  |  |  |  |  | **108** |  |  |  |  |  |
| **44** |  |  |  |  |  | **109** |  |  |  |  |  |
| **45** |  |  |  |  |  | **110** |  |  |  |  |  |
| **46** |  |  |  |  |  | **111** |  |  |  |  |  |
| **47** |  |  |  |  |  | **112** |  |  |  |  |  |
| **48** |  |  |  |  |  | **113** |  |  |  |  |  |
| **49** |  |  |  |  |  | **114** |  |  |  |  |  |
| **50** |  |  |  |  |  | **115** |  |  |  |  |  |
| **51** |  |  |  |  |  | **116** |  |  |  |  |  |
| **52** |  |  |  |  |  | **117** |  |  |  |  |  |
| **53** |  |  |  |  |  | **118** |  |  |  |  |  |
| **54** |  |  |  |  |  | **119** |  |  |  |  |  |
| **55** |  |  |  |  |  | **120** |  |  |  |  |  |
| **56** |  |  |  |  |  | **121** |  |  |  |  |  |
| **57** |  |  |  |  |  | **122** |  |  |  |  |  |
| **58** |  |  |  |  |  | **123** |  |  |  |  |  |
| **59** |  |  |  |  |  | **124** |  |  |  |  |  |
| **60** |  |  |  |  |  | **125** |  |  |  |  |  |
| **61** |  |  |  |  |  | **126** |  |  |  |  |  |
| **62** |  |  |  |  |  | **127** |  |  |  |  |  |
| **63** |  |  |  |  |  | **128** |  |  |  |  |  |
| **64** |  |  |  |  |  | **129** |  |  |  |  |  |
| **65** |  |  |  |  |  | **130** |  |  |  |  |  |

**CONTENTS**

[1.0 INTRODUCTION 4](#_Toc97969795)

[2.0 Scope 4](#_Toc97969796)

[3.0 NORMATIVE REFERENCES 5](#_Toc97969797)

[**3.1** **The Project Documents** 5](#_Toc97969798)

[**3.2** **ENVIRONMENTAL DATA** 5](#_Toc97969799)

[4.0 ELECTRICAL CONSUMPTION 6](#_Toc97969800)

1. **INTRODUCTION**

Binak oilfield in Bushehr province is a part of the southern oilfields of Iran, is located 20 km northwest of Genaveh city.

With the aim of increasing production of oil from Binak oilfield, an EPC/EPD Project has been defined by NIOC/NISOC and awarded to Petro Iran Development Company (PEDCO). Also PEDCO (as General Contractor) has assigned the EPC-packages of the Project to "Hirgan Energy - Design and Inspection" JV.

**GENERAL DEFINITION**

The following terms shall be used in this document.

|  |  |
| --- | --- |
| CLIENT:  | National Iranian South Oilfields Company (NISOC)  |
| PROJECT: | Binak Oilfield Development – Surface Facilities; New Gas Compressor Station |
| EPD/EPC CONTRACTOR:  | Petro Iran Development Company (PEDCO) |
| EPC CONTRACTOR: | Joint Venture of : Hirgan Energy – Design & Inspection(D&I) Companies |
| VENDOR: | The firm or person who will fabricate the equipment or material. |
| EXECUTOR:  | Executor is the party which carries out all or part of construction and/or commissioning for the project. |
| THIRD PARTY INSPECTOR (TPI): | The firm appointed by EPC CONTRACTOR and approved by GC & CLIENT (in writing) for the inspection of goods. |
| SHALL: | Is used where a provision is mandatory. |
| SHOULD: | Is used where a provision is advisory only. |
| WILL:  | Is normally used in connection with the action by CLIENT rather than by an EPC/EPD CONTRACTOR, supplier or VENDOR. |
| MAY:  | Is used where a provision is completely discretionary. |

1. **Scope**

The purpose of this document is to provide summary of process electrical loads for BINAK Gas Compressor Station”.

1. **NORMATIVE REFERENCES**

## **The Project Documents**

* BK-GNRAL-PEDCO-000-PR-DC-0001 Process Design Criteria
* BK-GNRAL-PEDCO-000-PR-DB-0001 Process Basis Of Design
* BK-GCS-PEDCO-120-PR-UF-0001 Utility Flow Diagrams (UFD)
* BK-GCS-PEDCO-120-PR-PI-0002~0025 P&ID
* BK-GCS-PEDCO-120-PR-PF-0001 Process Flow Diagram (PFD)

## **ENVIRONMENTAL DATA**

Refer to "Process Basis of Design; Doc. No. BK-GNRAL-PEDCO-000-PR-DB-0001".

1. **ELECTRICAL CONSUMPTION**

D03

| **No.** | **ITEM No.** | **SERVICE** | **C / I** | **Configuration** | **Emergency** | **N/S** | **Efficiency** | **POWER****(EACH)** |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **BHP (kW)** |
| 1 | AC-2101 A/B/C | 1st Stage Air Coolers | C | 2+1 | - | 2N+S | - | 8.5 (Each) (NOTE1) |
| 2 | AC-2102 A/B/C/ | 2nd  Stage Air Coolers | C | 2+1 | - | 2N+S | - | 19 (Each) (NOTE1) |
| 3 | C-2101 A/B/CC-2102 A/B/C | 1st & 2nd StageGas Compressor Package + Other Consumption | C | 2+1 | - | 2N+S | - | 484+448 (Each) |
| 4 | PK-C-2203 A/B | Instrument & Plant Air Package | C | 1+1 | E | N+S | - | 40 (NOTE1) |
| 5 | PK-Dr-2203 A/B | Air Dryer Package | C | 1+1 | - | N | - | 2 (NOTE1) |
| 6 | PK-C-2204 | Air compressor for N2 Package | C | 1 | - | N | - | 30 |
| 7 | PK-2204 | Nitrogen Package | C | 1 | - | N | - | 2 (NOTE1) |
| 8 | PK-2201 | LP Flare Package(Including blower for smokeless Flare) | C | 1 | - | N | - | 22.5 (NOTE1) |
| 9 | IG-2201 | LP Flare Ignition Package | I | 1 | E | N | - | 2 (NOTE1) |
| 10 | PK-2207 | Corrosion Inhibitor Package | C | 1 | - | N | - | 2 (NOTE1) |
| 11 | PK-2208 | Methanol Injection Package | DELETED |
| 12 | PK‐2101 | Dehydration Package | C | 1 | - | N | - | 20 (NOTE1) |
| 13 | P-2203A/B | Sump Pump | I | 1+1 | E | N+S | 31% | 1 |
| 14 | P-2202 A/B | Closed Drain Pumps | I | 1+1 |  E | N+S | 22% | 2.9 |
| 15 | P-2101A/B | Slug Pumps | I | 1+1 | E | N+S | 61% | 7 |
| 16 | P-2302 A/B | Fire Water Jockey Pumps | I | 1+1 | - | N+S | 29% | Rated power =14.8Motor Power =18.5 |
| 17 | P-2301 A | Fire Water electric Pump | I | 1 | - | N | 72% | Rated power =180.5Motor Power =250 |
| 18 | P-2209 | Potable Water Pumps | I | 1 | - | N | 31% | 1 |
| 19 | P-2206 | Diesel Oil Pump | I | 1 | - | N | 52% | 0.3 |
| 20 | P-2201A/B | LP Flare K.O. Drum Pumps | I | 1+1 | E | N+S | 15% | 0.6 |
| 21 | P-2103 A/B | Glycol Transfer Pumps | I | 1+1 | - | N+S | 31% | 1 |
| 22 | P-2102 | Glycol Manual Pump | I | 1 | - | N | 31% | 0.4 |
| 23 | P-2104 | Glycol Drain Pump | I | 1 | - | N | 22% | 0.8 |
| 24 | - | MOV | I | 2 |  - | N | - | 2(NOTE1) |
| 25 | Electrical tracing 1st Stage | 1st Stage Compressors | C | 2+1 | %85 | 2N+S | - | 0.227 |
| 26 | Electrical tracing 2nd Stage | 2nd Stage Compressors | C | 2+1 | %85 | 2N+S | - | 2.625 |

NOTE 1: Will be finalized by vendor.

C: Continues/ E: Emergency Load/ I: Intermittent/ N: Normal Load/ S: Standby