|  |
| --- |
| **طرح نگهداشت و افزایش تولید 27 مخزن** |
| **MTO FOR TRANSMISSION OVER HEAD LINE - BK14****نگهداشت و افزایش تولید میدان نفتی بینک** |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
| D01 | Nov. 2022 | IFI | H.Shakiba | M.Fakharian | M.Mehrshad |  |
| D00 | Sep. 2022 | IFI | H.Shakiba | M.Fakharian | M.Mehrshad |  |
| **Rev.** | **Date** | **Purpose of Issue/Status** | **Prepared by:** | **Checked by:** | **Approved by:** | **CLIENT Approval** |
| **Class: 3** | **CLIENT Doc. Number: F8Z-708199** |
| **Status:** | **IDC: Inter-Discipline Check****IFC: Issued For Comment** **IFA: Issued For Approval****AFD: Approved For Design** **AFC: Approved For Construction** **AFP: Approved For Purchase****AFQ: Approved For Quotation** **IFI: Issued For Information****AB-R: As-Built for Client Review** **AB-A: As-Built –Approved** |

**REVISION RECORD SHEET**

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **PAGE** | **D00** | **D01** | **D02** | **D03** | **D04** |  | **PAGE** | **D00** | **D01** | **D02** | **D03** | **D04** |
| **1** | X | X |  |  |  | **51** |  |  |  |  |  |
| **2** | X | X |  |  |  | **52** |  |  |  |  |  |
| **3** | X |  |  |  |  | **53** |  |  |  |  |  |
| **4** | X |  |  |  |  | **54** |  |  |  |  |  |
| **5** | X |  |  |  |  | **55** |  |  |  |  |  |
| **6** | X | X |  |  |  | **56** |  |  |  |  |  |
| **7** |  | X |  |  |  | **57** |  |  |  |  |  |
| **8** |  |  |  |  |  | **58** |  |  |  |  |  |
| **9** |  |  |  |  |  | **59** |  |  |  |  |  |
| **10** |  |  |  |  |  | **60** |  |  |  |  |  |
| **11** |  |  |  |  |  | **61** |  |  |  |  |  |
| **12** |  |  |  |  |  | **62** |  |  |  |  |  |
| **13** |  |  |  |  |  | **63** |  |  |  |  |  |
| **14** |  |  |  |  |  | **64** |  |  |  |  |  |
| **15** |  |  |  |  |  | **65** |  |  |  |  |  |
| **16** |  |  |  |  |  | **66** |  |  |  |  |  |
| **17** |  |  |  |  |  | **67** |  |  |  |  |  |
| **18** |  |  |  |  |  | **68** |  |  |  |  |  |
| **19** |  |  |  |  |  | **69** |  |  |  |  |  |
| **20** |  |  |  |  |  | **70** |  |  |  |  |  |
| **21** |  |  |  |  |  | **71** |  |  |  |  |  |
| **22** |  |  |  |  |  | **72** |  |  |  |  |  |
| **23** |  |  |  |  |  | **73** |  |  |  |  |  |
| **24** |  |  |  |  |  | **74** |  |  |  |  |  |
| **25** |  |  |  |  |  | **75** |  |  |  |  |  |
| **26** |  |  |  |  |  | **76** |  |  |  |  |  |
| **27** |  |  |  |  |  | **77** |  |  |  |  |  |
| **28** |  |  |  |  |  | **78** |  |  |  |  |  |
| **29** |  |  |  |  |  | **79** |  |  |  |  |  |
| **30** |  |  |  |  |  | **80** |  |  |  |  |  |
| **31** |  |  |  |  |  | **81** |  |  |  |  |  |
| **32** |  |  |  |  |  | **82** |  |  |  |  |  |
| **33** |  |  |  |  |  | **83** |  |  |  |  |  |
| **34** |  |  |  |  |  | **84** |  |  |  |  |  |
| **35** |  |  |  |  |  | **85** |  |  |  |  |  |
| **36** |  |  |  |  |  | **86** |  |  |  |  |  |
| **37** |  |  |  |  |  | **87** |  |  |  |  |  |
| **38** |  |  |  |  |  | **88** |  |  |  |  |  |
| **39** |  |  |  |  |  | **89** |  |  |  |  |  |
| **40** |  |  |  |  |  | **90** |  |  |  |  |  |
| **41** |  |  |  |  |  | **91** |  |  |  |  |  |
| **42** |  |  |  |  |  | **92** |  |  |  |  |  |
| **43** |  |  |  |  |  | **93** |  |  |  |  |  |
| **44** |  |  |  |  |  | **94** |  |  |  |  |  |
| **45** |  |  |  |  |  | **95** |  |  |  |  |  |
| **46** |  |  |  |  |  | **96** |  |  |  |  |  |
| **47** |  |  |  |  |  | **97** |  |  |  |  |  |
| **48** |  |  |  |  |  | **98** |  |  |  |  |  |
| **49** |  |  |  |  |  | **99** |  |  |  |  |  |
| **50** |  |  |  |  |  | **100** |  |  |  |  |  |

**CONTENTS**

[1.0 INTRODUCTION 4](#_Toc119422949)

[2.0 Scope 5](#_Toc119422950)

[3.0 NORMATIVE REFERENCES 5](#_Toc119422951)

[3.1 Local Codes and Standards 5](#_Toc119422952)

[3.2 International Codes and Standards 5](#_Toc119422953)

[3.3 The Project Documents 5](#_Toc119422954)

[3.4 ENVIRONMENTAL DATA 5](#_Toc119422955)

[4.0 ATTACHMENT1 (OHL MTO) 6](#_Toc119422956)

[5.0 ATTACHMENT2 (substation MTO) 7](#_Toc119422957)

1. **INTRODUCTION**

Binak oilfield in Bushehr province is a part of the southern oilfields of Iran, is located 20 km northwest of Genaveh city.

With the aim of increasing production of oil from Binak oilfield, an EPC/EPD Project has been defined by NIOC/NISOC and awarded to Petro Iran Development Company (PEDCO). Also PEDCO (as General Contractor) has assigned the EPC-packages of the Project to "Hirgan Energy - Design and Inspection" JV.

As a part of the Project, required modifications on BK14 workover well (with electric power supply) shall be done.

**GENERAL DEFINITION**

The following terms shall be used in this document.

|  |  |
| --- | --- |
| CLIENT:  | National Iranian South Oilfields Company (NISOC)  |
| PROJECT: | Binak Oilfield Development – Construction of Well Location, Wellhead Facilities, Electrification Facilities, & Flowlines for W046S  |
| EPD/EPC CONTRACTOR:  | Petro Iran Development Company (PEDCO) |
| EPC CONTRACTOR: | Joint Venture of : Hirgan Energy – Design & Inspection(D&I) Companies |
| VENDOR: | The firm or person who will fabricate the equipment or material. |
| EXECUTOR:  | Executor is the party which carries out all or part of construction and/or commissioning for the project. |
| THIRD PARTY INSPECTOR (TPI): | The firm appointed by EPC CONTRACTOR and approved by GC & Company (in writing) for the inspection of goods. |
| SHALL: | Is used where a provision is mandatory. |
| SHOULD: | Is used where a provision is advisory only. |
| WILL:  | Is normally used in connection with the action by COMPANY rather than by an EPC/EPD CONTRACTOR, supplier or VENDOR. |
| MAY:  | Is used where a provision is completely discretionary. |

1. **Scope**

This document covers the MTO for Over Head Line to BK-14.

It shall be used in conjunction with data/requisition sheets for present document subject.

1. **NORMATIVE REFERENCES**

## Local Codes and Standards

* IPS-E-EL-100 Engineering Standard for Electrical System Design
* IPS-E-EL-160 Engineering Standard for Overhead Transmission & Distribution Lines

## International Codes and Standards

* آیین نامه بارگذاری برج ها- جلد 50.211 استاندارد جامع مهندسی و طراحی خطوط انتقال نیروی برق ایران
* نقشه پهنه بندی کشور- جلد 50.221 استاندارد جامع مهندسی و طراحی خطوط انتقال نیروی برق ایران

## The Project Documents

* BK-BK14-PEDCO-110-SU-DW-0001 Over Head Line Plan and Profile – BK14
* BK-SSGRL-PEDCO-110-EL-RT-0005 33KV Over Head Line Study Report
* BK-SSGRL-PEDCO-110-EL-DT-0013 Data Sheets for 33 KV Over Head Line Equipment

## ENVIRONMENTAL DATA

Refer to "Electrical System Design Criteria”; Doc. No. “BK-GNRAL-PEDCO-000-EL-DC-0001".

1. **ATTACHMENT1 (OHL MTO)**

D01

| **MTO for Transmission Over Head Line - BK14** |
| --- |
| **Item** | **Description** | **Unit** | **Qty** |
|  | Basic Body with all accessories e.g., Stub, Legs, Anti-climbing thorn, Ladder, … for Lattice 1Circuit Tower – **Suspension** Type A | Set | 2 |
|  | Basic Body with all accessories e.g., Stub, Legs, Anti-climbing thorn, Ladder, … for Lattice 1Circuit Tower – **Tension** Type B | Set | 2 |
|  | Basic Body with all accessories e.g., Stub, Legs, Anti-climbing thorn, Ladder, … for Lattice 1Circuit Tower – **Dead End** **Tension** Type C | Set | 2 |
|  | Phase Conductor – ACSR/Hyena | m | 3000 |
|  | Shield Wire – 7No.8/AW | m | 1000 |
|  | 70 KN Porcelain/Ceramic Type Disc Insulator - 33kV | No. | 225 |
|  | 70 KN “I” Type Tension Accessories for Hyena Conductor | Set | 30 |
|  | 70 KN “I” Type Suspension Accessories for Hyena Conductor | Set | 6 |
|  | 70 KN “I” Type Jumper Accessories for Hyena Conductor | Set | 6 |
|  | Damper for Hyena Conductor | No. | 36 |
|  | Mid Span Joint for Hyena Conductor | No | 2 |
|  | Repair sleeve for Hyena Conductor | No | 1 |
|  | 70 KN Tension Accessories for 7No.8 | Set | 12 |
|  | 70 KN Suspension Accessories for 7No.8 | Set | 2 |
|  | Damper for 7No8AW | No | 12 |
|  | Mid Span Joint for 7No8AW | No | 1 |
|  | Repair sleeve for 7No8AW | No | 1 |
|  | Warning Colored ball with Armor rod for 7No.8 | Set | 2 |
|  | Danger & phase plate for towers | No | 6 |
|  | 35mm2 Copper Wire | m | 270 |
|  | Earthing Rod 1.5m-16mm | Set | 6 |
|  | Clamp for connecting the ground wire to the stub | Set | 24 |
|  | Clamp for connecting the ground wire to Rod | Set | 6 |
|  | Clamp for connecting the ground wire to ground wire | Set | 6 |

1. **ATTACHMENT2 (substation MTO)**

D01

| **MTO for substation (Gantry in T-off for BK14/Goreh/Binak and Gantry in well No. BK14)** |
| --- |
| **Item** | **Description** | **Unit** | **Qty** |
|  | Load Break Switch, 36kV, 630A, 25kA/1s (Outdoor Type) | Set | 5 |
|  | Earthing switch, Complete with manually operated mechanism | Set | 3 |
|  | Cut out fuse, 36kV, 3Phase | Set | 3 |
|  | Surge Arrester, 36kV, 10kA, Cl.2 | No. | 9 |
|  | 70kN Porcelain/Ceramic Type Disc Insulator - 33kV | No. | 105 |
|  | 36kV Post Insulator, Strength Class C6 | No. | 3 |
|  | 36kV Cable Sealing End, heat shrinkable, with lug and accessories | No. | 3 |
|  | Gantries with 2 column & 1 beam | Set | 5 |
|  | All beam & support & adaptor for MV equipment and fixing of them | Set | 5 |