|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **طرح نگهداشت و افزایش تولید 27 مخزن** | | | | | | |
| **EQUIPMENT LIST**  **نگهداشت و افزایش تولید میدان نفتی بینک** | | | | | | |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
| V01 | OCT. 2023 | IFR | Havayar Co. | M.Fakharian | S. Faramarzpour |  |
| V00 | MAY. 2023 | IFR | Havayar Co. | M.Fakharian | A.M.Mohseni |  |
| **Rev.** | **Date** | **Purpose of Issue/Status** | **Prepared by:** | **Checked by:** | **Approved by:** | **CLIENT Approval** |
|  | | | | | | |
| **Status:** | **IFA: Issued For Approval**  **IFR: Issued For Review**  **IFI: Issued For Information**  **AFC: Approved For Construction** | | | | | |

**REVISION RECORD SHEET**

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **PAGE** | **V00** | **V01** | **V02** | **V03** | **V04** |  | **PAGE** | **V00** | **V01** | **V02** | **V03** | **V04** |
| **1** | X | X |  |  |  | **66** |  |  |  |  |  |
| **2** | X | X |  |  |  | **67** |  |  |  |  |  |
| **3** | X |  |  |  |  | **68** |  |  |  |  |  |
| **4** | X |  |  |  |  | **69** |  |  |  |  |  |
| **5** | X | X |  |  |  | **70** |  |  |  |  |  |
| **6** |  | X |  |  |  | **71** |  |  |  |  |  |
| **7** |  |  |  |  |  | **72** |  |  |  |  |  |
| **8** |  |  |  |  |  | **73** |  |  |  |  |  |
| **9** |  |  |  |  |  | **74** |  |  |  |  |  |
| **10** |  |  |  |  |  | **75** |  |  |  |  |  |
| **11** |  |  |  |  |  | **76** |  |  |  |  |  |
| **12** |  |  |  |  |  | **77** |  |  |  |  |  |
| **13** |  |  |  |  |  | **78** |  |  |  |  |  |
| **14** |  |  |  |  |  | **79** |  |  |  |  |  |
| **15** |  |  |  |  |  | **80** |  |  |  |  |  |
| **16** |  |  |  |  |  | **81** |  |  |  |  |  |
| **17** |  |  |  |  |  | **82** |  |  |  |  |  |
| **18** |  |  |  |  |  | **83** |  |  |  |  |  |
| **19** |  |  |  |  |  | **84** |  |  |  |  |  |
| **20** |  |  |  |  |  | **85** |  |  |  |  |  |
| **21** |  |  |  |  |  | **86** |  |  |  |  |  |
| **22** |  |  |  |  |  | **87** |  |  |  |  |  |
| **23** |  |  |  |  |  | **88** |  |  |  |  |  |
| **24** |  |  |  |  |  | **89** |  |  |  |  |  |
| **25** |  |  |  |  |  | **90** |  |  |  |  |  |
| **26** |  |  |  |  |  | **91** |  |  |  |  |  |
| **27** |  |  |  |  |  | **92** |  |  |  |  |  |
| **28** |  |  |  |  |  | **93** |  |  |  |  |  |
| **29** |  |  |  |  |  | **94** |  |  |  |  |  |
| **30** |  |  |  |  |  | **95** |  |  |  |  |  |
| **31** |  |  |  |  |  | **96** |  |  |  |  |  |
| **32** |  |  |  |  |  | **97** |  |  |  |  |  |
| **33** |  |  |  |  |  | **98** |  |  |  |  |  |
| **34** |  |  |  |  |  | **99** |  |  |  |  |  |
| **35** |  |  |  |  |  | **100** |  |  |  |  |  |
| **36** |  |  |  |  |  | **101** |  |  |  |  |  |
| **37** |  |  |  |  |  | **102** |  |  |  |  |  |
| **38** |  |  |  |  |  | **103** |  |  |  |  |  |
| **39** |  |  |  |  |  | **104** |  |  |  |  |  |
| **40** |  |  |  |  |  | **105** |  |  |  |  |  |
| **41** |  |  |  |  |  | **106** |  |  |  |  |  |
| **42** |  |  |  |  |  | **107** |  |  |  |  |  |
| **43** |  |  |  |  |  | **108** |  |  |  |  |  |
| **44** |  |  |  |  |  | **109** |  |  |  |  |  |
| **45** |  |  |  |  |  | **110** |  |  |  |  |  |
| **46** |  |  |  |  |  | **111** |  |  |  |  |  |
| **47** |  |  |  |  |  | **112** |  |  |  |  |  |
| **48** |  |  |  |  |  | **113** |  |  |  |  |  |
| **49** |  |  |  |  |  | **114** |  |  |  |  |  |
| **50** |  |  |  |  |  | **115** |  |  |  |  |  |
| **51** |  |  |  |  |  | **116** |  |  |  |  |  |
| **52** |  |  |  |  |  | **117** |  |  |  |  |  |
| **53** |  |  |  |  |  | **118** |  |  |  |  |  |
| **54** |  |  |  |  |  | **119** |  |  |  |  |  |
| **55** |  |  |  |  |  | **120** |  |  |  |  |  |
| **56** |  |  |  |  |  | **121** |  |  |  |  |  |
| **57** |  |  |  |  |  | **122** |  |  |  |  |  |
| **58** |  |  |  |  |  | **123** |  |  |  |  |  |
| **59** |  |  |  |  |  | **124** |  |  |  |  |  |
| **60** |  |  |  |  |  | **125** |  |  |  |  |  |
| **61** |  |  |  |  |  | **126** |  |  |  |  |  |
| **62** |  |  |  |  |  | **127** |  |  |  |  |  |
| **63** |  |  |  |  |  | **128** |  |  |  |  |  |
| **64** |  |  |  |  |  | **129** |  |  |  |  |  |
| **65** |  |  |  |  |  | **130** |  |  |  |  |  |

**CONTENTS**

[1.0 INTRODUCTION 4](#_Toc133915328)

[2.0 Equipment List 5](#_Toc133915329)

1. **INTRODUCTION**

Binak oilfield in Bushehr province is a part of the southern oilfields of Iran, is located 20 km northwest of Genaveh city.

With the aim of increasing production of oil from Binak oilfield, an EPC/EPD Project has been defined by NIOC/NISOC and awarded to Petro Iran Development Company (PEDCO). Also, PEDCO (as General Contractor) has assigned the EPC-packages of the Project to "Hirgan Energy - Design and Inspection" JV.

**GENERAL DEFINITION**

The following terms shall be used in this document.

|  |  |
| --- | --- |
| CLIENT: | National Iranian South Oilfields Company (NISOC) |
| PROJECT: | Binak Oilfield Development – General Facilities |
| EPD/EPC CONTRACTOR (GC): | Petro Iran Development Company (PEDCO) |
| OWNER: | OWNER is collectively refer to National Iranian South Oil Company (NISOC) and Petro Iran Development Company (PEDCO) |
| EPC CONTRACTOR: | Joint Venture of: Hirgan Energy – Design & Inspection(D&I) Companies |
| VENDOR: | Havayar Company |
| EXECUTOR: | Executor is the party which carries out all or part of construction and/or commissioning for the project. |
| THIRD PARTY INSPECTOR (TPI): | The firm appointed by EPD/EPC CONTRACTOR (GC) and approved by CLIENT (in writing) for the inspection of goods. |
| SHALL: | Is used where a provision is mandatory. |
| SHOULD: | Is used where a provision is advisory only. |
| WILL: | Is normally used in connection with the action by CLIENT rather than by an EPC/EPD CONTRACTOR, supplier or VENDOR. |
| MAY: | Is used where a provision is completely discretionary. |
|  |  |
|  |  |

2. **Equipment List**

V01

| **Item** | **Equipment Description** | **Tag No.** | **Service** | **Operating Pressure (barg)** | | **Design Pressure (barg)** | | **Operating / Design Temp. (°C)** | | **QTY.** | **P&ID No.** | **Dimension (mm)** | **Material** | **C.A. (mm)** | **Insulation** | **Hazardous Area** | **Rated Capacity (kg/hr)** |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | 1st Stage Suction Snubber | C-2101-D1 A/B/C | Hydrocarbon | 4.9 | | 24.5 | | 36.8 / 180 | | 3 | BK-GCS-HY-120-PR-PI-0001 | TBD | A106 B / A234 WPB | 3 | Heat Traced | - | - |
|  | 1st Stage Discharge Snubber | C-2101-D2 A/B/C | Hydrocarbon | 18 | | 24.5 | | 129 / 180 | | 3 | BK-GCS-HY-120-PR-PI-0001 | TBD | A106 B / A234 WPB | 3 | Personnel Protection | - | - |
|  | 2nd Stage Suction Snubber | C-2102-D1 A/B/C | Hydrocarbon | 17.1 | | 62 | | 59.9 / 180 | | 3 | BK-GCS-HY-120-PR-PI-0001 | TBD | A106 B / A234 WPB | 3 | Heat Traced | - | - |
|  | 2nd Stage Discharge Snubber | C-2102-D2 A/B/C | Hydrocarbon | 54.9 | | 62 | | 147 / 180 | | 3 | BK-GCS-HY-120-PR-PI-0001 | TBD | A106 B / A234 WPB | 3 | Personnel Protection | - | - |
|  | Compressor | C-2101/2 A/B/C | Hydrocarbon | 1st stage | 4.8 / 18 | 1st stage | 24.5 | 1st stage | 36.8 / 180 | 3 | BK-GCS-HY-120-PR-PI-0001 | Width: 7925 | Details Acc. to Datasheet | - | - | - | 8935.5 |
| 2nd stage | 17 / 54.9 | 2nd stage | 62 | 2nd stage | 59.9 / 180 | 8935.5 |
|  | Main Oil Pump | P-2101-MP A/B/C | Lubrication Oil | 5 | | 8 | | 70 / 85 | | 3 | BK-GCS-HY-120-PR-PI-0001 | Length: 410  Dia.: 430 | Casing: A536 | - | - | Zone 2 | 6923.874 |
|  | Aux. Oil Pump | P-2101-AP A/B/C | Lubrication Oil | 5 | | 8 | | 70 / 85 | | 3 | BK-GCS-HY-120-PR-PI-0001 | TBD | TBD | - | - | Zone 2 | 6923.874 |
|  | Lube Oil Filter | F-2101-OF A/B/C | Lubrication Oil | 5 | | 8 | | 60 / 85 | | 6 | BK-GCS-HY-120-PR-PI-0001 | TBD | Element:  SS | 0 | - | - | - |
|  | Lube Oil Air Cooler | AE-2101-OC A/B/C | Lubrication Oil | 5 | | 8 | | 70 / 85 | | 3 | BK-GCS-HY-120-PR-PI-0001 | TBD | Stainless Steel | 0 | - | Zone 2 | TBD |
|  | Packing Leakage Collection Pot | V-2104 A/B/C | Nitrogen / Hydrocarbon | 1.5 | | 5 | | 60 / 85 | | 3 | BK-GCS-HY-120-PR-PI-0001 | TBD | A106 B / A234 WPB | 6 | Personnel Protection | - | - |
|  | Distance Piece Collecting Pot | V-2105 A/B/C | Nitrogen / Hydrocarbon | 1.5 | | 5 | | 60 / 85 | | 3 | BK-GCS-HY-120-PR-PI-0001 | TBD | A106 B / A234 WPB | 6 | Personnel Protection | - | - |
|  | Buffer Gas Filter | F-2101-BF A/B/C | Nitrogen | 7.5 | | 10 | | 60 / 85 | | 3 | BK-GCS-HY-120-PR-PI-0001 | TBD | Stainless Steel | - | - | Zone 2 | - |
|  | Main Water Pump | P-2101-WP A/B/C | Water | 3 | | 7 | | 65 / 85 | | 3 | BK-GCS-HY-120-PR-PI-0001 | TBD | Cast Iron | - | - | Zone 2 | TBD |
|  | Aux. Water Pump | P-2101-AX A/B/C | Water | 3 | | 7 | | 65 / 85 | | 3 | BK-GCS-HY-120-PR-PI-0001 | TBD | Cast Iron | - | - | Zone 2 | TBD |
|  | Water Air Cooler | AE-2101-WC A/B/C | Water | 3 | | 7 | | 65 / 85 | | 3 | BK-GCS-HY-120-PR-PI-0001 | TBD | Carbon Steel | TBD | - | Zone 2 | TBD |
|  | Cooling Water Filter | F-2101/02-WF A/B/C | Water | 3 | | 7 | | 58 / 85 | | 6 | BK-GCS-HY-120-PR-PI-0001 | TBD | TBD | - | Personnel Protection | - | - |
|  | Strainer | ST-2101/02 A/B/C | Hydrocarbon | 1st stage | 4.9 | 1st stage | 7 | 1st stage | 36.8 / 180 | 6 | BK-GCS-HY-120-PR-PI-0001 | TBD | Stainless Steel mesh | 3 | Heat Traced | - | - |
| 2nd stage | 17.1 | 2nd stage | 24.5 | 2nd stage | 59.9 / 180 |
|  | Electrical Oil Heater | H-2101-OH A/B/C | Lubrication Oil | ATM | | ATM | | 60 / 85 | | 3 | BK-GCS-HY-120-PR-PI-0001 | TBD | TBD | - | - | Zone 2 | - |
|  | Electrical Water Heater | H-2101-WH A/B/C | Water | ATM | | ATM | | 58 / 85 | | 3 | BK-GCS-HY-120-PR-PI-0001 | TBD | TBD | - | - | Zone 2 | - |
|  | Water Reservoir | TK-2101-WR A/B/C | Water | ATM | | ATM | | 58 / 85 | | 3 | BK-GCS-HY-120-PR-PI-0001 | 1.5 m3 | Carbon Steel | 3 | Personnel Protection | - | - |

V01

General Note:

TBD: To be determined.